**ROOFGRIP PRODUCT RANGE**

ROOFGRIP Modified Bituminous Membranes are manufactured to the highest level of industrial quality standards are offered for variety of exposed and concealed application.

**ROOFGRIP TORCH APPLIED MEMBRANES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Product | Grade | Thickness | Top Finish | Roll Size |
| PLASTOGRIP RL-500 (For Concealed Waterproofing) | RL-500 | 5.00 mm | Polyethylene Film | 1MX10M |
| PLASTOGRIP RL-400 (For Concealed Waterproofing) | RL-400 | 4.00 mm | Polyethylene Film | 1MX10M |
| PLASTOGRIP RL-300 (For Concealed Waterproofing) | RL-300 | 3.00 mm | Polyethylene Film | 1MX10M |
| PLASTOGRIP RLA-400 (For Exposed Waterproofing) | RLA-400 | 4.00 mm | Aluminum Foil | 1MX10M |
| PLASTOGRIP RLA-300 (For Exposed Waterproofing) | RLA-300 | 3.00 mm | Aluminum Foil | 1MX10M |
| PLASTOGRIP RLG-400 (Slated) (For Exposed Waterproofing) | RLG-400 | 4.00 mm | Slated | 1MX10M |
| PLASTOGRIP RLG-300 (Granules) (For Exposed Waterproofing) | RLG-300 | 3.00 mm | Granules | 1MX10M |

**ROOFGRIP SELF-ADHESIVE MEMBRANES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Product | Grade | Thickness | Top Finish | Roll Size |
| ELASTOGRIP RL-150 (For Concealed Waterproofing) | RL-150 | 1.5 mm | Polyethylene Film | 1MX15M |
| ELASTOGRIP RL-200 (For Concealed Waterproofing) | RL-200 | 2.00 mm | Polyethylene Film | 1MX15M |
| ELASTOGRIP RL-300 (For Concealed Waterproofing) | RL-300 | 3.00 mm | Polyethylene Film | 1MX10M |
| ELASTOGRIP RL-300 (SBS TOUCH ON) | RL-300 | 3.00 mm | Polyethylene Film | 1MX10M |
| ELASTOGRIP RL-400 (SBS TORCH ON) | RL-400 | 4.00 mm | Polyethylene Film | 1MX10M |

**ROOFGRIP APP TORCH APPLIED MEMBRANES**

The lower Surface is covered with Torchable Polyethylene Film.

**ROOFGRIP SBS SELF-ADHESIVE MEMBRANES**

The lower Surface is covered with Removable Film.